Real-Time Pothole Detection and Mapping System for SmartVehicles Using YOLOv8

Dharma Teja Garipally (22BCE8224) , Kowshik Annam (22BCE8333) , Ambati Sharanya Reddy (22BCE8396) , and Polisetti Govardhini(22BCE8163).

Computer Science and Engineering, Vellore Institute of Technology Amaravati, Andhra Pradesh, India [info@vitap.ac.in](mailto:info@vitap.ac.in)

**Abstract**

https://vitap.ac.in


This project aims to develop a system for automated and accurate pothole detection to improve road safety and maintenance efficiency. Potholes are a widespread issue that significantly impact road infrastructure, causing accidents, vehicle damage, and escalating repair costs. The current method of pothole detection, which relies on manual inspections, is labor-intensive, slow, and results in delays in repairs, leading to extended exposure to unsafe road conditions. Motivated by the limitations of traditional approaches, we plan to utilize advanced technologies such as image processing, machine learning, and deep learning algorithms to automate the detection of potholes. By employing these techniques, we aim to enhance the accuracy, reduce the time for identification, and ultimately improve the overall road maintenance process, ensuring safer roads and efficient resource allocation for repairs.


Keywords: Pothole detection, Deep Learning Architectures, YOLO, TensorFlow, Roboflow.

**Model Evaluation:**

The YOLOv8-Small model is characterized by its emphasis on faster inference speed achieved through a reduction in size. This design choice renders it well-suited for real- time applications where expeditious pothole detection takes precedence.

However, a potential drawback lies in its compromise on accuracy, particularly in discerning smaller potholes or those situated within complex backgrounds. In contrast, the YOLOv8- Medium strikes a balance between speed and accuracy, presenting a versatile option for reliable pothole detection across various scenarios. It occupies a middle ground, demonstrating adaptability without sacrificing essential accuracy. On the other hand, YOLOv8-Nano, renowned for its speed, sacrifices a degree of accuracy to maintain efficiency in real-time applications. This model excels in swiftly detecting larger potholes but may overlook finer details in the process.



Figure 1. YOLOv8 Model Structure

**Data Set:**

In this study, we use two extensive datasets for pothole detection. The first dataset includes over 1500 annotated images from Roboflow and an additional 1000 images sourced from various online platforms. The second dataset features over 1500 images captured from car dashboards and other sources, providing realistic road conditions from a driver’s perspective. Combined, these datasets total more than 3000 images, encompassing a wide range of scenarios and conditions. This diverse collection is instrumental for training and validating robust pothole detection models, ensuring comprehensive coverage and accuracy.

# Problem Statements:

Potholes are a common issue on roads worldwide, leading to significant safety hazards fordrivers and passengers alike. They contribute to accidents, vehicle damage, and increase the cost of road maintenance. Traditional methods of detecting potholes rely heavily on manual inspections, which are labor-intensive, time-consuming, and often result in delayed repairs. The inefficiencies in current practices lead to prolonged exposure to dangerous road conditions, making it imperative to develop a more effective solution.

# Proposed Solution:

This project proposes the development of an automated pothole detection system using the advanced YOLOv8 (You Only Look Once version 8) deep learning model. YOLOv8 is renowned for its speed and accuracy in object detection tasks, making it an ideal choicefor real-time pothole identification. The system will be designed to process video feeds or images captured by cameras mounted on vehicles or roadside infrastructure, identifyingand localizing potholes with high precision. The detected potholes will be marked and their coordinates will be recorded on a digital map, enabling quick response and targeted road maintenance efforts

# Expected Outcomes:

* A fully operational pothole detection system capable of identifying and localizingpotholes in real-time.
* A comprehensive mapping of detected potholes, allowing road maintenance teams toprioritize repairs based on severity and location.
* A reduction in road accidents and vehicle damage caused by potholes, leading toenhanced public safety and lower vehicle maintenance costs.

-A streamlined process for road monitoring and maintenance, reducing the time and resources needed for manual inspections.

# Conclusion:

This project presents a cutting-edge approach to improving road safety and maintenance efficiency through the use of deep learning technology. By automating the detection of potholes with YOLOv8, the system not only accelerates the identification process but also enhances the accuracy of pothole localization. The resulting solution is expected to significantly reduce the risks associated with potholes, lower the costs of vehicle repairs, and optimize the efforts of road maintenance teams. Ultimately, this project aims to contribute to safer and more reliable road infrastructure, benefiting both drivers and maintenance authorities.

**References:**

* + [1] O. o. I. R. a. Development, "Distress Identification Manual for the Long- TermPavement Performance Project," U.S Department of Transportation Federal Highway Administration, 2014.
  + [2] I. G. V. P. Heggie, "Commercial Management and Financing of Roads," WorldBank, Washington, 1998.
  + [3] A. M. Legreid, "Potholes and Strategies on the Road to Campus Internationalization," International Research and Review: Journal of Phi Beta DeltaHonor Society for International Scholars, vol. 6, no. 1, 2016.
  + [4] A. F. Rita Justo-Silva, "Pavement maintenance considering traffic accidentcosts," International Journal of Pavement Research and Technology, 2019.
  + [5] S.-K. R. Taehyeong Kim, "A Guideline for Pothole Classification,”International Journal of Engineering and Technology, vol. 4, 2014.
  + [6] B. X. Yu and X. Yu, "Vibration-Based System for Pavement Condition Evaluation," in Applications of Advanced Technology in Transportation, 2006.
  + [7] K. D. Zoysa, G. P. Seneviratne, W. W. A. T. Shihan and C. Keppitiyagama, "A Public Transport System Based Sensor Network for Road Surface Condition Monitoring," in SIGCOMM07: ACM SIGCOMM 2007 Conference, Kyoto, 2007.
  + [8] L. G. B. H. R. N. S. M. H. B. Jakob Eriksson, "The Pothole Patrol: Using aMobile Sensor Network for Road Surface Monitoring," in

Mobisys08: The 6thInternational Conference on Mobile Systems, Applications, and Services, Breckenridge, 2008.

* + [9] K. C. P. Wang, "Challenges and Feasibility for Comprehensive Automated Survey of Pavement Conditions," in Eighth International Conference on Applications of Advanced Technologies in Transportation Engineering (AATTE),Beijing, 2004.
  + [10] K. T. Chang, J. R. Chang and J. K. Liu, "Detection of Pavement Distresses Using 3D Laser Scanning Technology," in International Conference on Computingin Civil Engineering 2005, Cancun, 2005.
  + [11] Z. Hou, K. C. Wang and W. Gong, "Experimentation of 3d Pavement Imaging Through Stereovision," in International Conference on Transportation Engineering 2007, Chengdu, 2007.
  + [12] C. Koch and I. Brilakis, "Pothole detection in asphalt pavement images,"Advanced Engineering Informatics, vol. 25, no. 3, pp. 507- 515, 2011.
  + [13] G. M. Jog, C. Koch, M. Golparvar-Fard and I. Brilakis, “Pothole PropertiesMeasurement through Visual 2D Recognition and 3D Reconstruction," in International Conference on Computing in Civil Engineering, Florida, 2012.
  + [14] L. Huidrom, L. K. Das and S. Sud, "Method for automated assessment of potholes, cracks and patches from road surface video clips,” Procedia - Social andBehavioral Sciences, vol. 104, pp. 312-321, 2013.
  + [15] Aparna, Y. Bhatia, R. Rai, V. Gupta, N. Aggarwal and A. Akula, "Convolutional neural networks based potholes detection using thermal imaging,"Journal of King Saud University – Computer and Information Sciences, 2019.
  + [16] A. Bianchini, P. Bandini and D. W. Smith, "Interrater Reliability of Manual Pavement Distress Evaluations," Journal of Transportation Engineering, vol. 136,no. 2, pp. 165-172, 2010.
  + [17] O. Mendoza, P. Melin and G. Licea, "A New Method for Edge Detection in Image Processing using Interval Type-2 Fuzzy Logic," in 2007 IEEE InternationalConference on Granular Computing, California, 2007.
  + [18] T. Kim and S.-K. Ryu, "Review and analysis of pothole detection methods," Journal of Emerging Trends in Computing and Information Sciences, vol. 5, no. 8,pp. 603-608, 2014.
  + [19] A. Bhat, P. Narkar, D. Shetty and D. Vyas, "Detection of Potholes using ImageProcessing Techniques," IOSR Journal of Engineering, vol. 2, pp. 52-56, 2018.
  + [20] M. Muslim, D. Sulistyaningrum and B. Setiyono, "Detection and countingpotholes using morphological method from road video," AIP Conference Proceedings, vol. 2242, no. 1, pp. 3-11, 2020.
  + [21] Z. Zhang, X. Ai, C. Chan and N. Dahnoun, "An efficient algorithm for potholedetection using stereo vision," 2014 IEEE International Conference on Acoustics, Speech and Signal Processing (ICASSP), pp. 564-568, 2014.
  + [22] Y. Jo and S. Ryu, "Pothole detection system using a black-box camera,"Sensors, vol. 15, no. 11, pp. 29316-29331, 2015.
  + [23] T. Kim and S.-K. Ryu, "Intelligent compaction terminal system for asphalt pavement in Korea," J. Emerg. Trends Comput. Inform. Sci, vol. 6, pp. 154-158,2015.
  + [24] T. a. R. S. Kim, "Pothole DB based on 2D images and video data," J. Emerg.Trends Comput. Inform. Sci, vol. 5, pp. 527-531, 2014.
  + [25] S. Nienaber, M. Booysen and R. Kroon, "Detecting Potholes Using SimpleImage Processing Techniques And Real-World Footage," in South African Transport Conference, Pretoria, 2015.