Real-Time Pothole Detection and Mapping System for SmartVehicles Using YOLOv8

Dharma Teja Garipally (22BCE8224) , Kowshik Annam (22BCE8333) , Ambati Sharanya Reddy (22BCE8396) , and Polisetti Govardhini(22BCE8163).

Computer Science and Engineering, Vellore Institute of Technology Amaravati, Andhra Pradesh, India [info@vitap.ac.in](mailto:info@vitap.ac.in)

**Abstract**

https://vitap.ac.in

This project aims to develop a system for automated and accurate pothole detection to improve road safety and maintenance efficiency. Potholes are a widespread issue that significantly impact road infrastructure, causing accidents, vehicle damage, and escalating repair costs. The current method of pothole detection, which relies on manual inspections, is labor-intensive, slow, and results in delays in repairs, leading to extended exposure to unsafe road conditions. Motivated by the limitations of traditional approaches, we plan to utilize advanced technologies such as image processing, machine learning, and deep learning algorithms to automate the detection of potholes. By employing these techniques, we aim to enhance the accuracy, reduce the time for identification, and ultimately improve the overall road maintenance process, ensuring safer roads and efficient resource allocation for repairs.

Keywords: Pothole detection, Deep Learning Architectures, YOLO, TensorFlow, Roboflow.

**Model Evaluation:**

The YOLOv8-Small model is characterized by its emphasis on faster inference speed achieved through a reduction in size. This design choice renders it well-suited for real- time applications where expeditious pothole detection takes precedence.

However, a potential drawback lies in its compromise on accuracy, particularly in discerning smaller potholes or those situated within complex backgrounds. In contrast, the YOLOv8- Medium strikes a balance between speed and accuracy, presenting a versatile option for reliable pothole detection across various scenarios. It occupies a middle ground, demonstrating adaptability without sacrificing essential accuracy. On the other hand, YOLOv8-Nano, renowned for its speed, sacrifices a degree of accuracy to maintain efficiency in real-time applications. This model excels in swiftly detecting larger potholes but may overlook finer details in the process.





Figure 1. YOLOv8 Model Structure

**Data Set:**

In this study, we use two extensive datasets for pothole detection. The first dataset includes over 1500 annotated images from Robo flow and an additional 1000 images sourced from various online platforms. The second dataset features over 1500 images captured from car dashboards and other sources, providing realistic road conditions from a driver’s perspective. Combined, these datasets total more than 3000 images, encompassing a wide range of scenarios and conditions. This diverse collection is instrumental for training and validating robust pothole detection models, ensuring comprehensive coverage and accuracy.

# Problem Statements:

Potholes are a common issue on roads worldwide, leading to significant safety hazards for drivers and passengers alike. They contribute to accidents, vehicle damage, and increase the cost of road maintenance. Traditional methods of detecting potholes rely heavily on manual inspections, which are labor-intensive, time-consuming, and often result in delayed repairs. The inefficiencies in current practices lead to prolonged exposure to dangerous road conditions, making it imperative to develop a more effective solution.

# Proposed Solution:

This project proposes the development of an automated pothole detection system using the advanced YOLOv8 (You Only Look Once version 8) deep learning model. YOLOv8 is renowned for its speed and accuracy in object detection tasks, making it an ideal choice for real-time pothole identification. The system will be designed to process video feeds or images captured by cameras mounted on vehicles or roadside infrastructure, identifying and localizing potholes with high precision. The detected potholes will be marked and their coordinates will be recorded on a digital map, enabling quick response and targeted road maintenance efforts

# Expected Outcomes:

* A fully operational pothole detection system capable of identifying and localizing potholes in real-time.
* A comprehensive mapping of detected potholes, allowing road maintenance teams to prioritize repairs based on severity and location.
* A reduction in road accidents and vehicle damage caused by potholes, leading to enhanced public safety and lower vehicle maintenance costs.

- A streamlined process for road monitoring and maintenance, reducing the time and resources needed for manual inspections.

**Requirement Analysis for the Pothole Detection System**

1. **Functional Requirements:**

- **Real-Time Pothole Detection:** The system must detect potholes in real-time using YOLOv8. It should be capable of processing video streams from vehicle-mounted cameras or other sources to identify and localize potholes.

- **Pothole Localization and Mapping:** The system should provide the exact geolocation (latitude and longitude) of detected potholes and mark them on a digital map. This mapping will assist road maintenance teams in identifying and prioritizing repairs.

- **Data Acquisition and Preprocessing:** The system will collect images or video data of roads, which will be preprocessed and fed into the YOLOv8 model. The preprocessing will involve tasks such as noise reduction, resizing, and image augmentation.

- **Classification and Reporting:** The detected potholes should be categorized based on size or severity, and the system should generate periodic reports for road maintenance authorities. The system must also have the capability to notify users of newly detected potholes in specific locations.

**2. Non-Functional Requirements:**

- **Performance:** The system should have low latency to ensure real-time pothole detection. It should be optimized for speed, ensuring minimal impact on vehicle performance and road monitoring systems.

- **Accuracy:** The detection system should maintain a high level of accuracy, with an acceptable false-positive rate, especially under various weather and lighting conditions.

- **Scalability:** The system should be scalable to process large datasets and multiple video streams simultaneously, making it suitable for deployment across multiple vehicles or road monitoring systems in large cities.

- **Usability:** The interface for displaying pothole locations and generating reports should be user-friendly, allowing road maintenance teams to easily interpret the data.

- **Reliability:** The system must be reliable and capable of functioning in diverse environmental conditions, including different weather scenarios and road conditions.

- **Security:** The system should ensure that the data related to pothole detection, especially location-based information, is protected against unauthorized access and tampering.

**Literature Survey: Pothole Detection Using YOLOv8**

**1. Pothole Detection Techniques Using Deep Learning**

In recent years, the application of deep learning techniques to pothole detection has gained considerable momentum, thanks to advancements in real-time object detection models like YOLO (You Only Look Once). YOLO models, particularly the latest iterations such as YOLOv8, offer high accuracy with efficient processing speeds, making them ideal for real-time applications like pothole detection in smart vehicles.

Several research works highlight the use of deep learning, especially YOLO, for real-time road condition monitoring:

- Ali et al. (2021) proposed a system utilizing YOLOv7 for pothole detection, with a focus on real-time classification and localization of road anomalies. The study demonstrated YOLOv7's ability to balance speed and accuracy, which is vital for real-time monitoring【13†source】.

- Seung et al. (2015) developed an image-based pothole detection system utilizing a black-box camera mounted on vehicles, contributing to the advancement of automated road monitoring systems【14†source】.

- Rastogi et al. (2020) compared multiple deep learning algorithms, including Convolutional Neural Networks (CNNs), for detecting road damage and potholes. Their findings highlighted YOLO's efficiency in handling large-scale video data for real-time applications【14†source】【15†source】.

These studies establish that YOLO, specifically YOLOv8, is highly capable of identifying potholes with accuracy and speed, positioning it as a practical choice for large-scale pothole detection systems.

**2. Comparison of YOLOv8 with Other Models**

The YOLOv8 model, being the most recent and optimized version of YOLO, is designed for real-time object detection with smaller model sizes, allowing for faster inference speeds. However, a trade-off exists between speed and detection accuracy, particularly for smaller objects or in complex environments. Various versions of YOLOv8 offer different balances:

- YOLOv8-Nano: Optimized for speed, this model is highly effective in detecting larger potholes but may miss smaller ones or those in difficult conditions. This makes it suitable for scenarios where quick detection is essential but might struggle in highly detailed environments.

- YOLOv8-Medium: Strikes a balance between speed and accuracy, making it versatile for a variety of road conditions. It is well-suited for detecting potholes in environments with varying lighting and road surface complexity.

The main advantage of YOLOv8 over its predecessors (YOLOv3, YOLOv4) is its lighter architecture, which allows it to process real-time video feeds in high resolution while maintaining efficiency, making it highly suitable for vehicle-mounted applications.

**3. Pothole Detection Using Other Technologies**

Prior to the widespread adoption of deep learning models like YOLO, traditional image processing and sensor-based techniques were predominantly used for pothole detection:

- Kim and Ryu (2014) proposed a guideline for classifying potholes using traditional image processing techniques like edge detection and segmentation.

- Yu and Salari (2011) employed vibration-based and laser imaging methods to evaluate pavement conditions. These methods required specialized sensors and had limited real-time capabilities.

While these methods were foundational, their reliance on specialized hardware and their inability to handle large-scale, real-time data limited their application. The introduction of deep learning models, particularly YOLO, has resolved many of these limitations by providing a scalable and efficient approach for detecting road anomalies in real-time, with just the use of video cameras.

**4. Dataset Utilization**

Data quality and diversity are critical in training robust deep learning models. For this project, two comprehensive datasets are utilized:

- Roboflow Dataset: This dataset consists of over 1500 annotated images sourced from various online platforms. It includes images of potholes under varying lighting and environmental conditions, making it valuable for training YOLOv8 to detect potholes under different scenarios.

- Dashboard Camera Dataset: This dataset contains over 1500 images captured from vehicle dashboard cameras. It provides real-world data with a focus on the driver’s perspective, enhancing the model’s ability to generalize to real-time conditions.

These datasets, diverse in their environmental contexts, are instrumental in ensuring the model’s ability to detect potholes in real-time, regardless of weather, lighting, or road type. Moreover, the integration of these datasets ensures that the model can adapt to various driving conditions, thereby improving its robustness.

**5. YOLO’s Role in Pothole Detection: A Comparative Study**

Comparing various versions of YOLO, researchers have shown that:

- YOLOv3 was highly efficient in real-time object detection but required more processing power compared to later versions like YOLOv7 and YOLOv8.

- YOLOv7 and YOLOv8 demonstrated faster inference speeds with comparable accuracy, making them suitable for real-time pothole detection, as demonstrated in works by Sathvik et al. (2022) and Gajjar et al. (2022).

In recent studies, models such as YOLOv5 and YOLOv8 were tested across various terrains and environmental conditions. Hoseini et al. (2023) introduced a smart solution using YOLOv5 to detect and track potholes with satellite positioning, which helped improve road maintenance planning.

From the literature surveyed, it is evident that deep learning models, particularly YOLO variants, are at the forefront of pothole detection technology. YOLOv8 stands out for its optimized architecture, providing a balance between detection speed and accuracy. The use of robust datasets enhances the model's performance across diverse road conditions. This integration of real-time object detection technology into smart vehicles ensures more efficient road monitoring, which is critical for future smart city infrastructure.

YOLOv8 offers a powerful solution for real-time pothole detection, making it possible to process large-scale video data and report anomalies accurately. This literature survey underlines the importance of using YOLOv8 to optimize both road safety and maintenance processes, demonstrating its practical application in various scenarios globally.

# Conclusion:

This project presents a cutting-edge approach to improving road safety and maintenance efficiency through the use of deep learning technology. By automating the detection of potholes with YOLOv8, the system not only accelerates the identification process but also enhances the accuracy of pothole localization. The resulting solution is expected to significantly reduce the risks associated with potholes, lower the costs of vehicle repairs, and optimize the efforts of road maintenance teams. Ultimately, this project aims to contribute to safer and more reliable road infrastructure, benefiting both drivers and maintenance authorities.

**References:**

* + [1] O. o. I. R. a. Development, "Distress Identification Manual for the Long- TermPavement Performance Project," U.S Department of Transportation Federal Highway Administration, 2014.
  + [2] I. G. V. P. Heggie, "Commercial Management and Financing of Roads," WorldBank, Washington, 1998.
  + [3] A. M. Legreid, "Potholes and Strategies on the Road to Campus Internationalization," International Research and Review: Journal of Phi Beta DeltaHonor Society for International Scholars, vol. 6, no. 1, 2016.
  + [4] A. F. Rita Justo-Silva, "Pavement maintenance considering traffic accidentcosts," International Journal of Pavement Research and Technology, 2019.
  + [5] S.-K. R. Taehyeong Kim, "A Guideline for Pothole Classification,”International Journal of Engineering and Technology, vol. 4, 2014.
  + [6] B. X. Yu and X. Yu, "Vibration-Based System for Pavement Condition Evaluation," in Applications of Advanced Technology in Transportation, 2006.
  + [7] K. D. Zoysa, G. P. Seneviratne, W. W. A. T. Shihan and C. Keppitiyagama, "A Public Transport System Based Sensor Network for Road Surface Condition Monitoring," in SIGCOMM07: ACM SIGCOMM 2007 Conference, Kyoto, 2007.

[8] L. G. B. H. R. N. S. M. H. B. Jakob Eriksson, "The Pothole Patrol: Using aMobile Sensor Network for Road Surface Monitoring," inMobisys08: The 6thInternational Conference on Mobile Systems, Applications, and Services, Breckenridge, 2008.

* + [9] K. C. P. Wang, "Challenges and Feasibility for Comprehensive Automated Survey of Pavement Conditions," in Eighth International Conference on Applications of Advanced Technologies in Transportation Engineering (AATTE), Beijing, 2004.
  + [10] K. T. Chang, J. R. Chang and J. K. Liu, "Detection of Pavement Distresses Using 3D Laser Scanning Technology," in International Conference on Computing in Civil Engineering 2005, Cancun, 2005.
  + [11] Z. Hou, K. C. Wang and W. Gong, "Experimentation of 3d Pavement Imaging Through Stereovision," in International Conference on Transportation Engineering 2007, Chengdu, 2007.
  + [12] C. Koch and I. Brilakis, "Pothole detection in asphalt pavement images," Advanced Engineering Informatics, vol. 25, no. 3, pp. 507- 515, 2011.
  + [13] G. M. Jog, C. Koch, M. Golparvar-Fard and I. Brilakis, “Pothole Properties Measurement through Visual 2D Recognition and 3D Reconstruction," in International Conference on Computing in Civil Engineering, Florida, 2012.
  + [14] L. Huidrom, L. K. Das and S. Sud, "Method for automated assessment of potholes, cracks and patches from road surface video clips,” Procedia - Social and Behavioral Sciences, vol. 104, pp. 312-321, 2013.
  + [15] Aparna, Y. Bhatia, R. Rai, V. Gupta, N. Aggarwal and A. Akula, "Convolutional neural networks based potholes detection using thermal imaging," Journal of King Saud University – Computer and Information Sciences, 2019.
  + [16] A. Bianchini, P. Bandini and D. W. Smith, "Interrater Reliability of Manual Pavement Distress Evaluations," Journal of Transportation Engineering, vol. 136, no. 2, pp. 165-172, 2010.
  + [17] O. Mendoza, P. Melin and G. Licea, "A New Method for Edge Detection in Image Processing using Interval Type-2 Fuzzy Logic," in 2007 IEEE International Conference on Granular Computing, California, 2007.
  + [18] T. Kim and S.-K. Ryu, "Review and analysis of pothole detection methods," Journal of Emerging Trends in Computing and Information Sciences, vol. 5, no. 8, pp. 603-608, 2014.
  + [19] A. Bhat, P. Narkar, D. Shetty and D. Vyas, "Detection of Potholes using Image Processing Techniques," IOSR Journal of Engineering, vol. 2, pp. 52-56, 2018.
  + [20] M. Muslim, D. Sulistyaningrum and B. Setiyono, "Detection and counting potholes using morphological method from road video," AIP Conference Proceedings, vol. 2242, no. 1, pp. 3-11, 2020.